| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
WDT peripheral driver configuration
WDT driver

## Macros
#define | WDT_ENABLED
| Enable WDT driver * Set to 1 to activate. More...
#define | WDT_CONFIG_BEHAVIOUR
| WDT behavior in CPU SLEEP or HALT mode * Following options are avaiable: More...
#define | WDT_CONFIG_RELOAD_VALUE
| Reload value * Minimum value: 15 Maximum value: 4294967295. More...
#define | WDT_CONFIG_IRQ_PRIORITY
| Interrupt priority. More...

## Detailed Description

## Macro Definition Documentation

#define WDT_CONFIG_BEHAVIOUR

WDT behavior in CPU SLEEP or HALT mode * Following options are avaiable:

- 1 - Run in SLEEP, Pause in HALT
- 8 - Pause in SLEEP, Run in HALT
- 9 - Run in SLEEP and HALT
- 0 - Pause in SLEEP and HALT

Note
  This is an NRF_CONFIG macro.

#define WDT_CONFIG_IRQ_PRIORITY

Interrupt priority.

Priorities 0,2 (nRF51) and 0,1,4,5 (nRF52) are reserved for SoftDevice

Following options are avaiable:

- 0 - 0 (highest)
- 1 - 1
- 2 - 2
- 3 - 3
- 4 - 4 (except nRF51 family)
- 5 - 5 (except nRF51 family)
- 6 - 6 (except nRF51 family)
- 7 - 7 (except nRF51 family)

Note
  This is an NRF_CONFIG macro.

#define WDT_CONFIG_RELOAD_VALUE

Reload value * Minimum value: 15 Maximum value: 4294967295.

Note
  This is an NRF_CONFIG macro.

#define WDT_ENABLED

Enable WDT driver * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.