| S212 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_radio_request_normal_t Struct Reference
Structures

Parameters for a normal radio timeslot request. More...

`#include <nrf_soc.h>`

## Data Fields
uint8_t | hfclk
uint8_t | priority
uint32_t | distance_us
uint32_t | length_us

## Detailed Description

Parameters for a normal radio timeslot request.

## Field Documentation

uint32_t nrf_radio_request_normal_t::distance_us

Distance from the start of the previous radio timeslot (up to NRF_RADIO_DISTANCE_MAX_US microseconds).

uint8_t nrf_radio_request_normal_t::hfclk

High frequency clock source, see NRF_RADIO_HFCLK_CFG.

uint32_t nrf_radio_request_normal_t::length_us

The radio timeslot length (in the range [100..100,000] microseconds).

uint8_t nrf_radio_request_normal_t::priority

The radio timeslot priority, see NRF_RADIO_PRIORITY.