| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_ias_s Struct Reference
Immediate Alert Service

Immediate Alert Service structure. This contains various status information for the service. More...

`#include <ble_ias.h>`

## Data Fields
ble_ias_evt_handler_t | evt_handler
uint16_t | service_handle
ble_gatts_char_handles_t | alert_level_handles
uint16_t | conn_handle

## Detailed Description

Immediate Alert Service structure. This contains various status information for the service.

## Field Documentation

ble_gatts_char_handles_t ble_ias_s::alert_level_handles

Handles related to the Alert Level characteristic.

uint16_t ble_ias_s::conn_handle

Handle of the current connection (as provided by the BLE stack, is BLE_CONN_HANDLE_INVALID if not in a connection).

ble_ias_evt_handler_t ble_ias_s::evt_handler

Event handler to be called for handling events in the Immediate Alert Service.

uint16_t ble_ias_s::service_handle

Handle of Immediate Alert Service (as provided by the BLE stack).