| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gattc_evt_attr_info_disc_rsp_t Struct Reference
Structures

Event structure for BLE_GATTC_EVT_ATTR_INFO_DISC_RSP. More...

`#include <ble_gattc.h>`

## Data Fields
uint16_t | count
uint8_t | format
union {
ble_gattc_attr_info16_t attr_info16 [1]
ble_gattc_attr_info128_t attr_info128 [1]
} | info

## Detailed Description

Event structure for BLE_GATTC_EVT_ATTR_INFO_DISC_RSP.

## Field Documentation

ble_gattc_attr_info128_t ble_gattc_evt_attr_info_disc_rsp_t::attr_info128[1]

     Attribute information for 128-bit Attribute UUID.

Note
  This is a variable length array. The size of 1 indicated is only a placeholder for compilation. See sd_ble_evt_get for more information on how to use event structures with variable length array members.

ble_gattc_attr_info16_t ble_gattc_evt_attr_info_disc_rsp_t::attr_info16[1]

      Attribute information for 16-bit Attribute UUID.

Note
  This is a variable length array. The size of 1 indicated is only a placeholder for compilation. See sd_ble_evt_get for more information on how to use event structures with variable length array members.

uint16_t ble_gattc_evt_attr_info_disc_rsp_t::count

Attribute count.

uint8_t ble_gattc_evt_attr_info_disc_rsp_t::format

Attribute information format, see Attribute Information Formats.

union { ... } ble_gattc_evt_attr_info_disc_rsp_t::info

Attribute information union.