| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_radio_request_earliest_t Struct Reference
Structures

Parameters for a request for a timeslot as early as possible. More...

`#include <nrf_soc.h>`

## Data Fields
uint8_t | hfclk
uint8_t | priority
uint32_t | length_us
uint32_t | timeout_us

## Detailed Description

Parameters for a request for a timeslot as early as possible.

## Field Documentation

uint8_t nrf_radio_request_earliest_t::hfclk

High frequency clock source, see NRF_RADIO_HFCLK_CFG.

uint32_t nrf_radio_request_earliest_t::length_us

The radio timeslot length (in the range 100 to 100,000] microseconds).

uint8_t nrf_radio_request_earliest_t::priority

The radio timeslot priority, see NRF_RADIO_PRIORITY.

uint32_t nrf_radio_request_earliest_t::timeout_us

Longest acceptable delay until the start of the requested timeslot (up to NRF_RADIO_EARLIEST_TIMEOUT_MAX_US microseconds).