| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Flash handling library
This information applies to the following SoftDevices: S130, S132, S332

This driver allows writing to the non-volatile memory (NVM) regions of the nRF5. In order to write to NVM the controller must be powered on and the relevant page must be erased.