| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - r -

- r0 : HardFault_stack
- r1 : HardFault_stack
- r12 : HardFault_stack
- r2 : HardFault_stack
- r3 : HardFault_stack
- racp : nrf_ble_cgms_char_handler_t
- racp_data : ble_cgms_s
- racp_handles : ble_gls_s
- racp_proc_operator : nrf_ble_cgms_racp_t
- racp_proc_record_ndx : nrf_ble_cgms_racp_t
- racp_proc_records_reported : nrf_ble_cgms_racp_t
- racp_proc_records_reported_since_txcomplete : nrf_ble_cgms_racp_t
- radio_irq_priority : nrf_esb_config_t
- ram_size : nrf_ic_info_t
- ratio : nrf_drv_i2s_config_t
- read_access : ble_add_char_user_desc_t , ble_add_char_params_t , ble_add_descr_params_t , type_2_tag_capability_container_t
- read_perm : ble_srv_security_mode_t , ble_srv_cccd_security_mode_t
- read_pos : app_fifo_t
- read_resp : ble_hids_inp_rep_init_t , ble_hids_outp_rep_init_t , ble_hids_feature_rep_init_t
- read_value : nrf_drv_csense_evt_t
- record_count : nfc_ndef_msg_desc_t
- record_id : fds_header_t , fds_record_desc_t
- record_is_open : fds_record_desc_t
- record_key : fds_tl_t
- ref_handle : ble_hids_rep_char_t
- reference : nrf_drv_adc_channel_config_t , nrf_drv_comp_config_t , nrf_adc_config_t , nrf_comp_ref_conf_t , nrf_lpcomp_config_t
- release_event : bsp_button_event_cfg_t
- reliable : nrf_drv_rtc_config_t
- reload_value : nrf_drv_wdt_config_t
- remaining_dist_present : ble_lns_navigation_s
- remaining_distance : ble_lns_navigation_s
- remaining_vert_dist_present : ble_lns_navigation_s
- remaining_vert_distance : ble_lns_navigation_s
- rep_index : ble_hids_char_id_t
- rep_map : ble_hids_init_t
- rep_map_ext_rep_ref_handle : ble_hids_s
- rep_map_handles : ble_hids_s
- rep_ref : ble_hids_inp_rep_init_t , ble_hids_outp_rep_init_t , ble_hids_feature_rep_init_t
- rep_type : ble_hids_char_id_t
- repeats : nrf_pwm_sequence_t
- report : nrf_drv_qdec_event_t
- report_id : ble_srv_report_ref_t
- report_ref_handle : ble_bas_s
- report_type : ble_srv_report_ref_t
- reportper : nrf_drv_qdec_config_t
- req_len : nrf_dfu_req_t
- req_opcode : ble_socp_rsp_t
- req_type : nrf_dfu_req_t
- required_feature : ant_encrypt_adv_burst_settings_t
- res_len : nrf_dfu_res_t
- reserved : ble_ans_alert_settings_t , nrf_drv_adc_channel_config_t , antfs_beacon_status_byte1_t , ant_bsc_page5_data_t
- resolution : nrf_drv_adc_channel_config_t , nrf_adc_config_t , nrf_drv_saadc_config_t
- resp_val : ble_socp_rsp_t
- response : ble_sc_ctrlpt_s
- result : fds_evt_t
- retransmit_count : nrf_esb_config_t
- retransmit_delay : nrf_esb_config_t
- rev_count : ant_bsc_page0_data_t
- rf_freq : ant_channel_config_t
- rolling_time : ble_lns_loc_speed_s
- rolling_time_present : ble_lns_loc_speed_s
- rr_interval : ble_hrs_s
- rr_interval_count : ble_hrs_s
- rsc : ble_rscs_c_evt_t
- rsc_cccd_handle : ble_rscs_c_db_t
- rsc_feature_attr_md : ble_rscs_init_t
- rsc_handle : ble_rscs_c_db_t
- rsc_meas_attr_md : ble_rscs_init_t
- rscs_db : ble_rscs_c_evt_t
- rsp_code : ble_lncp_rsp_t , ble_socp_rsp_t
- rssi : nrf_gzll_device_tx_info_t , nrf_esb_payload_t , nrf_gzll_host_rx_info_t
- rts_pin_no : app_uart_comm_params_t
- rx_amount : nrf_drv_spis_event_t , nrf_drv_twis_evt_t
- rx_buf : app_uart_buffers_t
- rx_buf_size : app_uart_buffers_t
- rx_handles : ble_nus_s
- rx_length : nrf_drv_spi_xfer_desc_t
- rx_pin_no : app_uart_comm_params_t
- rxtx : nrf_drv_uart_event_t , nrf_drv_uart_error_evt_t