| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Functions
Functions
Master Boot Record API

## Functions
uint32_t | sd_mbr_command (sd_mbr_command_t *param)
| Issue Master Boot Record commands. More...

## Detailed Description

## Function Documentation

uint32_t sd_mbr_command | ( | sd_mbr_command_t * | param | ) |

Issue Master Boot Record commands.

Commands used when updating a SoftDevice and bootloader.

Parameters

  [in] | param | Pointer to a struct describing the command.

Note
  for retvals see sd_mbr_command_copy_sd_t sd_mbr_command_copy_bl_t sd_mbr_command_compare_t