| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
low_power_pwm_config_t Struct Reference
Low-power PWM

Structure holding the initialization parameters. More...

`#include <low_power_pwm.h>`

## Data Fields
bool | active_high
uint8_t | period
uint32_t | bit_mask
app_timer_id_t const * | p_timer_id

## Detailed Description

Structure holding the initialization parameters.

## Field Documentation

bool low_power_pwm_config_t::active_high

Activate negative polarity.

uint32_t low_power_pwm_config_t::bit_mask

Pins to be initialized.

app_timer_id_t const* low_power_pwm_config_t::p_timer_id

Pointer to the timer ID of low_power_pwm.

uint8_t low_power_pwm_config_t::period

Width of the low_power_pwm period.