| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_dfu_s Struct Reference
Buttonless DFU Service

## Data Fields
uint8_t | uuid_type
uint16_t | service_handle
uint16_t | conn_handle
ble_gatts_char_handles_t | control_point_char
bool | is_ctrlpt_notification_enabled
ble_dfu_evt_handler_t | evt_handler
bool | is_waiting_for_disconnection

## Field Documentation

ble_gatts_char_handles_t ble_dfu_s::control_point_char

Handles related to the DFU Control Point characteristic.

ble_dfu_evt_handler_t ble_dfu_s::evt_handler

Event handler which is called right before.

uint16_t ble_dfu_s::service_handle

Handle of DFU (as provided by the SoftDevice).

uint8_t ble_dfu_s::uuid_type

UUID type for DFU UUID.