| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages

### - c -

- c : ble_gap_lesc_oob_data_t
- callback_action : nrf_radio_signal_callback_return_param_t
- cccd_handle : ble_gatts_char_handles_t
- central_conn_count : ble_gap_enable_params_t
- central_sec_count : ble_gap_enable_params_t
- ch_37_off : ble_gap_adv_ch_mask_t
- ch_38_off : ble_gap_adv_ch_mask_t
- ch_39_off : ble_gap_adv_ch_mask_t
- ch_map : ble_gap_opt_ch_map_t , ble_gap_opt_t
- channel_mask : ble_gap_adv_params_t
- char_disc_rsp : ble_gattc_evt_t
- char_ext_props : ble_gattc_char_t , ble_gatts_char_md_t
- char_props : ble_gatts_char_md_t , ble_gattc_char_t
- char_user_desc_max_size : ble_gatts_char_md_t
- char_user_desc_size : ble_gatts_char_md_t
- char_val_by_uuid_read_rsp : ble_gattc_evt_t
- char_vals_read_rsp : ble_gattc_evt_t
- chars : ble_gattc_evt_char_disc_rsp_t
- cid : ble_l2cap_header_t
- ciphertext : nrf_ecb_hal_data_t
- cleartext : nrf_ecb_hal_data_t
- command : sd_mbr_command_t
- common_enable_params : ble_enable_params_t
- common_evt : ble_evt_t
- common_opt : ble_opt_t
- company_id : ble_version_t
- compare : sd_mbr_command_t
- compat_mode : ble_gap_opt_t
- conn_bw : ble_common_opt_conn_bw_t , ble_common_opt_t
- conn_bw_rx : ble_conn_bw_t
- conn_bw_tx : ble_conn_bw_t
- conn_handle : ble_common_evt_t , ble_gap_evt_t , ble_gap_opt_ch_map_t , ble_gattc_evt_t , ble_gatts_evt_t , ble_l2cap_evt_t , ble_gap_opt_local_conn_latency_t
- conn_param_update : ble_gap_evt_t
- conn_param_update_request : ble_gap_evt_t
- conn_params : ble_gap_evt_connected_t , ble_gap_evt_conn_param_update_request_t , ble_gap_evt_conn_param_update_t
- conn_sec : ble_gap_evt_conn_sec_update_t
- conn_sec_update : ble_gap_evt_t
- conn_sup_timeout : ble_gap_conn_params_t
- connected : ble_gap_evt_t
- copy_bl : sd_mbr_command_t
- copy_sd : sd_mbr_command_t
- count : ble_gattc_evt_char_val_by_uuid_read_rsp_t , ble_evt_tx_complete_t , ble_gattc_evt_rel_disc_rsp_t , ble_gattc_evt_prim_srvc_disc_rsp_t , ble_gattc_evt_desc_disc_rsp_t , ble_gattc_evt_char_disc_rsp_t , ble_gattc_evt_attr_info_disc_rsp_t
- csrk : ble_gap_sign_info_t