| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Cycling Speed and Cadence Service
This information applies to the following SoftDevices: S130, S132, S332

This module implements the Cycling Speed and Cadence Service. If enabled, notification of the Cycling Speead and Candence Measurement is performed when the application calls ble_cscs_measurement_send().

If an event handler is supplied by the application, the Cycling Speed and Cadence Service will generate Cycling Speed and Cadence Service events to the application.

Note
  The application must propagate BLE stack events to the Cycling Speead and Candence Service module by calling ble_cscs_on_ble_evt() from the SoftDevice Event Handler function.