| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_evt_adv_report_t Struct Reference
Structures

Event structure for BLE_GAP_EVT_ADV_REPORT. More...

`#include <ble_gap.h>`

## Data Fields
ble_gap_addr_t | peer_addr
int8_t | rssi
uint8_t | scan_rsp: 1
uint8_t | type: 2
uint8_t | dlen: 5
uint8_t | data [31]

## Detailed Description

Event structure for BLE_GAP_EVT_ADV_REPORT.

## Field Documentation

uint8_t ble_gap_evt_adv_report_t::data[31]

Advertising or scan response data.

uint8_t ble_gap_evt_adv_report_t::dlen

Advertising or scan response data length.

ble_gap_addr_t ble_gap_evt_adv_report_t::peer_addr

Bluetooth address of the peer device.

int8_t ble_gap_evt_adv_report_t::rssi

Received Signal Strength Indication in dBm.

uint8_t ble_gap_evt_adv_report_t::scan_rsp

If 1, the report corresponds to a scan response and the type field may be ignored.

uint8_t ble_gap_evt_adv_report_t::type

See GAP Advertising types. Only valid if the scan_rsp field is 0.