| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Desktop device emulator
The Gazell protocol is considered experimental for the nRF52 Series.

This project can be used as a starting point for developing a nRF5 Series mouse or keyboard using Gazell for communicating with a legacy nRF24LU1 USB dongle. It can communicate "out of the box" with the Dongle reference design and the nRFreadySimplePairing.exe application, that can be found in the nRFready Desktop v1.2.3.

This project sends mouse movement packets to the USB dongle when pin 1 is low (button connected to pin 1 pressed) and sends the 'a' keyboard character to the USB dongle when pin 2 goes from high to low (button connected to pin 2 pressed).

You can find the source code and the project file of the example in the following folder: `<InstallFolder>\examples\proprietary_rf\gzll\gzp_desktop_emulator`