| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_advdata_conn_int_t Struct Reference
Advertising and Scan Response Data Encoder

Connection interval range structure. More...

`#include <ble_advdata.h>`

## Data Fields
uint16_t | min_conn_interval
uint16_t | max_conn_interval

## Detailed Description

Connection interval range structure.

## Field Documentation

uint16_t ble_advdata_conn_int_t::max_conn_interval

Maximum connection interval, in units of 1.25 ms, range 6 to 3200 (7.5 ms to 4 s). The value 0xFFFF indicates no specific maximum.

uint16_t ble_advdata_conn_int_t::min_conn_interval

Minimum connection interval, in units of 1.25 ms, range 6 to 3200 (7.5 ms to 4 s).