| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_radio_signal_callback_return_param_t Struct Reference
Structures

Return parameters of the radio timeslot signal callback. More...

`#include <nrf_soc.h>`

## Data Fields
uint8_t | callback_action
union {
struct {
nrf_radio_request_t * p_next
} request
struct {
uint32_t length_us
} extend
} | params

## Detailed Description

Return parameters of the radio timeslot signal callback.

## Field Documentation

uint8_t nrf_radio_signal_callback_return_param_t::callback_action

The action requested by the application when returning from the signal callback, see NRF_RADIO_SIGNAL_CALLBACK_ACTION.

struct { ... } nrf_radio_signal_callback_return_param_t::extend

Additional parameters for return_code NRF_RADIO_SIGNAL_CALLBACK_ACTION_EXTEND.

uint32_t nrf_radio_signal_callback_return_param_t::length_us

Requested extension of the radio timeslot duration (microseconds) (for minimum time see NRF_RADIO_MINIMUM_TIMESLOT_LENGTH_EXTENSION_TIME_US).

nrf_radio_request_t* nrf_radio_signal_callback_return_param_t::p_next

The request parameters for the next radio timeslot.

union { ... } nrf_radio_signal_callback_return_param_t::params

Parameter union.

struct { ... } nrf_radio_signal_callback_return_param_t::request

Additional parameters for return_code NRF_RADIO_SIGNAL_CALLBACK_ACTION_REQUEST_AND_END.