| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Common ANT stack configuration configuration
ANT stack configuration

## Macros
#define | ANT_STACK_CONFIG_ENABLED
| Enable ANT stack configuration. * Set to 1 to activate. More...
#define | ANT_CONFIG_TOTAL_CHANNELS_ALLOCATED
| Allocated ANT channels *. More...
#define | ANT_CONFIG_ENCRYPTED_CHANNELS
| Encrypted ANT channels *. More...
#define | ANT_CONFIG_EVENT_QUEUE_SIZE
| Event queue size *. More...
#define | ANT_CONFIG_BURST_QUEUE_SIZE
| ANT burst queue size *. More...

## Detailed Description

## Macro Definition Documentation

#define ANT_CONFIG_BURST_QUEUE_SIZE

ANT burst queue size *.

Note
  This is an NRF_CONFIG macro.

#define ANT_CONFIG_ENCRYPTED_CHANNELS

Encrypted ANT channels *.

Note
  This is an NRF_CONFIG macro.

#define ANT_CONFIG_EVENT_QUEUE_SIZE

Event queue size *.

Note
  This is an NRF_CONFIG macro.

#define ANT_CONFIG_TOTAL_CHANNELS_ALLOCATED

Allocated ANT channels *.

Note
  This is an NRF_CONFIG macro.

#define ANT_STACK_CONFIG_ENABLED

Enable ANT stack configuration. * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.