| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Privacy modes
Peer Manager

## Macros
#define | BLE_GAP_PRIVACY_MODE_OFF 0x00
#define | BLE_GAP_PRIVACY_MODE_DEVICE_PRIVACY 0x01

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_PRIVACY_MODE_DEVICE_PRIVACY 0x01

Device will send and accept only private addresses for its own address.

#define BLE_GAP_PRIVACY_MODE_OFF 0x00

Device will send and accept its identity address for its own address.