| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
sensorsim_cfg_t Struct Reference
Sensor Data Simulator

Triangular waveform sensor simulator configuration. More...

`#include <sensorsim.h>`

## Data Fields
uint32_t | min
uint32_t | max
uint32_t | incr
bool | start_at_max

## Detailed Description

Triangular waveform sensor simulator configuration.

## Field Documentation

uint32_t sensorsim_cfg_t::incr

Increment between each measurement.

uint32_t sensorsim_cfg_t::max

Maximum simulated value.

uint32_t sensorsim_cfg_t::min

Minimum simulated value.

bool sensorsim_cfg_t::start_at_max

TRUE is measurement is to start at the maximum value, FALSE if it is to start at the minimum.