| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_ble_cgms_meas_t Struct Reference
Structures

CGM measurement. More...

`#include <nrf_ble_cgms.h>`

## Data Fields
uint8_t | flags
uint16_t | glucose_concentration
uint16_t | time_offset
nrf_ble_cgms_sensor_annunc_t | sensor_status_annunciation
uint16_t | trend
uint16_t | quality

## Detailed Description

CGM measurement.

## Field Documentation

uint8_t nrf_ble_cgms_meas_t::flags

Indicates the presence of optional fields and the Sensor Status Annunciation field.

uint16_t nrf_ble_cgms_meas_t::glucose_concentration

Glucose concentration. 16-bit word comprising 4-bit exponent and signed 12-bit mantissa.

uint16_t nrf_ble_cgms_meas_t::quality

Optional field that includes the Quality of the measurement.

nrf_ble_cgms_sensor_annunc_t nrf_ble_cgms_meas_t::sensor_status_annunciation

Sensor Status Annunciation. Variable length, can include Status, Cal/Temp, and Warning.

uint16_t nrf_ble_cgms_meas_t::time_offset

Time offset. Represents the time difference between measurements.

uint16_t nrf_ble_cgms_meas_t::trend

Optional field that can include Trend Information.