| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
antfs_beacon_status_byte1_t Union Reference
ANT-FS client device simulator

ANT-FS beacon status. More...

`#include <antfs.h>`

## Data Fields
uint32_t | status
struct {
uint32_t link_period: 3
bool is_pairing_enabled: 1
bool is_upload_enabled: 1
bool is_data_available: 1
bool reserved: 2
} | parameters

## Detailed Description

ANT-FS beacon status.

## Field Documentation

bool antfs_beacon_status_byte1_t::is_data_available

Data is available for download / no data available.

bool antfs_beacon_status_byte1_t::is_pairing_enabled

Pairing is enabled/disabled.

bool antfs_beacon_status_byte1_t::is_upload_enabled

Upload is enabled/disabled.

uint32_t antfs_beacon_status_byte1_t::link_period

Beacon period (0.5 - 8 Hz).

bool antfs_beacon_status_byte1_t::reserved

Reserved.

uint32_t antfs_beacon_status_byte1_t::status

Beacon status byte 1.