| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Gazell
The Gazell protocol is considered experimental for the nRF52 Series.

Gazell for the nRF5 Series is a lightweight, low power, and easy-to-use protocol with advanced coexistence features especially suited for wireless desktop products and other power-sensitive wireless applications. It is on-air compatible with Gazell on Nordic's nRF24Lxx ICs, and can share an nRF5 Series device with a Nordic SoftDevice.

The following example applications show how to use the Gazell protocol:

- Device/Host example
- Desktop device emulator
- Pairing Device with Dynamic Pairing