| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_scan_params_t Struct Reference
Structures

GAP scanning parameters. More...

`#include <ble_gap.h>`

## Data Fields
uint8_t | active: 1
uint8_t | selective: 1
ble_gap_whitelist_t * | p_whitelist
uint16_t | interval
uint16_t | window
uint16_t | timeout

## Detailed Description

GAP scanning parameters.

## Field Documentation

uint8_t ble_gap_scan_params_t::active

If 1, perform active scanning (scan requests).

uint16_t ble_gap_scan_params_t::interval

Scan interval between 0x0004 and 0x4000 in 0.625ms units (2.5ms to 10.24s).

ble_gap_whitelist_t* ble_gap_scan_params_t::p_whitelist

Pointer to whitelist, NULL if no whitelist or the current active whitelist is to be used.

uint8_t ble_gap_scan_params_t::selective

If 1, ignore unknown devices (non whitelisted).

uint16_t ble_gap_scan_params_t::timeout

Scan timeout between 0x0001 and 0xFFFF in seconds, 0x0000 disables timeout.

uint16_t ble_gap_scan_params_t::window

Scan window between 0x0004 and 0x4000 in 0.625ms units (2.5ms to 10.24s).