| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
ANT Continuous Waveform Mode
This example requires the following SoftDevice: S212

Important: Before you run this example, make sure to program the SoftDevice.

The ANT CW Mode example is designed to show how to initialize the continuous waveform mode for certification testing using the ANT SoftDevice.

This example can be used with a single module in RF testing.

Continuous waveform mode broadcast

# Setup

You can find the source code and the project file of the example in the following folder: `<InstallFolder>\examples\ant\ant_cw_mode`

# Testing

Note: You can use a custom channel or encryption when running any of the ANT examples. When adding a new channel or encryption, remember to update ANT stack configuration.

1. Compile and program the Continuous Waveform Mode application onto the module.
2. This will run a modulated waveform at 2410MHz and +4dBm output power for doing wireless certification testing. You will require proper equipment for the testing, such as spectrum analyzers and anechoic chambers.