| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ant_sdm_page22_data_t Struct Reference
Stride Based Speed and Distance Monitor profile page 22

Data structure for SDM data page 22. More...

`#include <ant_sdm_page_22.h>`

## Data Fields
union {
struct {
bool time_is_valid: 1
| Transmitted time is valid.
bool distance_is_valid: 1
| Transmitted distance is valid.
bool speed_is_valid: 1
| Transmitted speed is valid.
bool latency_is_valid: 1
| Transmitted latency is valid.
bool cadency_is_valid: 1
| Transmitted cadency is valid.
bool calorie_is_valid: 1
| Transmitted calorie is valid.
} items
uint8_t byte
} | capabilities

## Detailed Description

Data structure for SDM data page 22.