| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Adafruit PN532 implementation for nRF5x configuration
Adafruit PN532 NFC Shield library

## Macros
#define | ADAFRUIT_PN532_ENABLED
| Enabling PN532 module * Set to 1 to activate. More...
#define | PN532_IRQ
| Pin number * Minimum value: 0 Maximum value: 31. More...
#define | PN532_RESET
| Pin number * Minimum value: 0 Maximum value: 31. More...
#define | PN532_CONFIG_SCL
| Pin number * Minimum value: 0 Maximum value: 31. More...
#define | PN532_CONFIG_SDA
| Pin number * Minimum value: 0 Maximum value: 31. More...
#define | PN532_CONFIG_TWI_INSTANCE
| TWI instance to be used * Following options are avaiable: More...

## Detailed Description

## Macro Definition Documentation

#define ADAFRUIT_PN532_ENABLED

Enabling PN532 module * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define PN532_CONFIG_SCL

Pin number * Minimum value: 0 Maximum value: 31.

Note
  This is an NRF_CONFIG macro.

#define PN532_CONFIG_SDA

Pin number * Minimum value: 0 Maximum value: 31.

Note
  This is an NRF_CONFIG macro.

#define PN532_CONFIG_TWI_INSTANCE

TWI instance to be used * Following options are avaiable:

- 0
- 1
- 2

Note
  This is an NRF_CONFIG macro.

#define PN532_IRQ

Pin number * Minimum value: 0 Maximum value: 31.

Note
  This is an NRF_CONFIG macro.

#define PN532_RESET

Pin number * Minimum value: 0 Maximum value: 31.

Note
  This is an NRF_CONFIG macro.