| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_radio_request_t Struct Reference
Structures

Radio timeslot request parameters. More...

`#include <nrf_soc.h>`

## Data Fields
uint8_t | request_type
union {
nrf_radio_request_earliest_t earliest
nrf_radio_request_normal_t normal
} | params

## Detailed Description

Radio timeslot request parameters.

## Field Documentation

nrf_radio_request_earliest_t nrf_radio_request_t::earliest

Parameters for requesting a radio timeslot as early as possible.

nrf_radio_request_normal_t nrf_radio_request_t::normal

Parameters for requesting a normal radio timeslot.

union { ... } nrf_radio_request_t::params

Parameter union.

uint8_t nrf_radio_request_t::request_type

Type of request, see NRF_RADIO_REQUEST_TYPE.