| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_pwm_values_t Union Reference
PWM HAL

Union grouping pointers to arrays of duty cycle values applicable to various loading modes. More...

`#include <nrf_pwm.h>`

## Data Fields
nrf_pwm_values_common_t const * | p_common
| Pointer to be used in NRF_PWM_LOAD_COMMON mode.
nrf_pwm_values_grouped_t const * | p_grouped
| Pointer to be used in NRF_PWM_LOAD_GROUPED mode.
nrf_pwm_values_individual_t const * | p_individual
| Pointer to be used in NRF_PWM_LOAD_INDIVIDUAL mode.
nrf_pwm_values_wave_form_t const * | p_wave_form
| Pointer to be used in NRF_PWM_LOAD_WAVE_FORM mode.
uint16_t const * | p_raw
| Pointer providing raw access to the values.

## Detailed Description

Union grouping pointers to arrays of duty cycle values applicable to various loading modes.