| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Pairing failure: Confirm failed
Peripheral Legacy Pairing

This occurs if the random value doesn't match, usually because the user entered a wrong pin or out of band data was missing.