| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_ancs_c_evt_notif_attr_t Struct Reference
Apple Notification Service client

iOS notification attribute structure for incomming attributes. More...

`#include <ble_ancs_c.h>`

## Data Fields
uint32_t | notif_uid
uint16_t | attr_len
ble_ancs_c_notif_attr_id_values_t | attr_id
uint8_t * | p_attr_data

## Detailed Description

iOS notification attribute structure for incomming attributes.

## Field Documentation

ble_ancs_c_notif_attr_id_values_t ble_ancs_c_evt_notif_attr_t::attr_id

Classification of the attribute type, for example, title or date.

uint16_t ble_ancs_c_evt_notif_attr_t::attr_len

Length of the received attribute data.

uint32_t ble_ancs_c_evt_notif_attr_t::notif_uid

UID of the notification that the attribute belongs to.

uint8_t* ble_ancs_c_evt_notif_attr_t::p_attr_data

Pointer to where the memory is allocated for storing incoming attributes.