| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_nus_init_t Struct Reference
Nordic UART Service

Nordic UART Service initialization structure. More...

`#include <ble_nus.h>`

## Data Fields
ble_nus_data_handler_t | data_handler

## Detailed Description

Nordic UART Service initialization structure.

This structure contains the initialization information for the service. The application must fill this structure and pass it to the service using the ble_nus_init function.

## Field Documentation

ble_nus_data_handler_t ble_nus_init_t::data_handler

Event handler to be called for handling received data.