| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - s -

- sample : nrf_drv_adc_sample_evt_t , nrf_drv_adc_evt_t , nrf_drv_qdec_event_t
- sample_inten : nrf_drv_qdec_config_t
- sample_location : ble_gls_meas_t , nrf_ble_cgms_feature_t
- sample_width : nrf_drv_i2s_config_t
- sampleper : nrf_drv_qdec_config_t
- sc_ctrlpt_attr_md : ble_cs_ctrlpt_init_t
- sc_ctrlpt_handles : ble_sc_ctrlpt_s
- scaling : nrf_adc_config_t
- sck_pin : nrf_drv_i2s_config_t , nrf_drv_spi_config_t , nrf_drv_spis_config_t
- scl : nrf_drv_twis_config_t , nrf_drv_twi_config_t
- scl_pull : nrf_drv_twis_config_t
- sd_size : nrf_dfu_settings_t
- sda : nrf_drv_twi_config_t , nrf_drv_twis_config_t
- sda_pull : nrf_drv_twis_config_t
- sdin_pin : nrf_drv_i2s_config_t
- sdout_pin : nrf_drv_i2s_config_t
- search_priority : ant_search_config_t
- search_sharing_cycles : ant_search_config_t
- secondary_length : nrf_drv_twi_xfer_desc_t
- security_mode : ble_hids_hid_information_t , ble_hids_inp_rep_init_t , ble_hids_outp_rep_init_t , ble_hids_feature_rep_init_t , ble_hids_rep_map_init_t
- security_mode_boot_kb_inp_rep : ble_hids_init_t
- security_mode_boot_kb_outp_rep : ble_hids_init_t
- security_mode_boot_mouse_inp_rep : ble_hids_init_t
- security_mode_ctrl_point : ble_hids_init_t
- security_mode_protocol : ble_hids_init_t
- selective_auto_ack : nrf_esb_config_t
- sense : nrf_drv_gpiote_in_config_t
- sensor_loc_handles : ble_cscs_s
- sensor_location : ble_cscs_init_t
- sensor_location_handle : ble_cs_ctrlpt_init_t , ble_sc_ctrlpt_s
- sensor_status : ble_cgms_s
- sensor_status_annunciation : ble_gls_meas_t , nrf_ble_cgms_meas_t
- sensor_type : ant_bpwr_simulator_cfg_t
- sensorsim_c_cfg : ant_bsc_simulator_cb_t
- sensorsim_c_state : ant_bsc_simulator_cb_t
- sensorsim_cfg : ant_hrm_simulator_cfg_t , ant_hrm_simulator_cb_t , ant_sdm_simulator_cfg_t , ant_sdm_simulator_cb_t
- sensorsim_s_cfg : ant_bsc_simulator_cb_t
- sensorsim_s_state : ant_bsc_simulator_cb_t
- sensorsim_state : ant_hrm_simulator_cb_t , ant_sdm_simulator_cb_t
- sequence_number : ble_gls_meas_t
- serial_num : ant_bsc_page2_data_t , ant_hrm_page2_data_t
- serial_num_str : ble_dis_init_t
- serial_number : ant_common_page81_data_t
- serial_number_part_1 : type_2_tag_serial_number_t
- serial_number_part_2 : type_2_tag_serial_number_t
- service : ble_ancs_c_service_t , ble_ancs_c_evt_t , ble_ancs_c_t , ble_ans_c_service_t , ble_ans_c_evt_t , ble_ans_c_s
- service_data_count : ble_advdata_t
- service_handle : ble_ans_c_s , ble_bas_s , ble_bps_s , ble_cscs_s , ble_dfu_t , ble_cs_ctrlpt_init_t , ble_sc_ctrlpt_s , ble_dfu_s , ble_tps_t , ble_gls_s , ble_hids_s , ble_hrs_s , ble_hts_s , ble_ias_s , ble_lbs_s , ble_lls_s , ble_nus_s , ble_rscs_s , ble_lns_s , nrf_ble_bms_s , ble_cgms_s
- service_uuid : ble_ias_c_s , ble_advdata_service_data_t
- services : ble_db_discovery_t
- session_run_time : ble_cgms_s
- settings : ble_ans_c_evt_t
- settings_version : nrf_dfu_settings_t
- short_name_len : ble_advdata_t
- silent : ble_ancs_c_notif_flags_t
- size : uint8_array_t , ble_add_char_user_desc_t , nrf_drv_adc_done_evt_t , nrf_drv_saadc_done_evt_t
- size_list_supported_locations : ble_cscs_init_t , ble_cs_ctrlpt_init_t , ble_sc_ctrlpt_s
- size_val : ble_socp_rsp_t
- slider : nrf_csense_evt_param_t
- sn : type_2_tag_t
- socp : nrf_ble_cgms_char_handler_t
- socp_response : ble_cgms_s
- speed : ant_sdm_common_data_t
- speed_event_time : ant_bsc_combined_page0_data_t
- speed_is_valid : ant_sdm_page22_data_t
- speed_mode : nrf_drv_comp_config_t
- speed_rev_count : ant_bsc_combined_page0_data_t
- speed_sim_val : ant_bsc_simulator_cb_t
- SPI_CPHA : spi_master_config_t
- SPI_CPOL : spi_master_config_t
- SPI_Freq : spi_master_config_t
- SPI_ORDER : spi_master_config_t
- SPI_Pin_MISO : spi_master_config_t
- SPI_Pin_MOSI : spi_master_config_t
- SPI_Pin_SCK : spi_master_config_t
- SPI_Pin_SS : spi_master_config_t
- srt : nrf_ble_cgms_char_handler_t
- srv_count : ble_db_discovery_t
- srv_uuid : ble_gatt_db_srv_t
- ss_pin : nrf_drv_spi_config_t
- sst : nrf_ble_cgms_char_handler_t
- stack_info : ble_error_log_data_t
- start_at_max : sensorsim_cfg_t
- start_on_notify_cccd_handle : ble_conn_params_init_t
- state : ant_request_controller_t , ant_sdm_page2_data_t
- status : nrf_ble_cgm_status_t , ble_sc_ctrlpt_resp_t , antfs_beacon_status_byte1_t , nrf_ble_cgms_sensor_annunc_t , ant_sdm_page2_data_t , nrf_ble_cgms_char_handler_t
- step : nrf_csense_slider_evt_t
- step_mode : nrf_drv_pwm_config_t
- stop_cnt : ant_bsc_simulator_cb_t
- stop_indicator : ant_bsc_page5_data_t
- stride_incr : ant_sdm_simulator_cb_t
- stride_length : ant_sdm_simulator_cb_t , ant_sdm_simulator_cfg_t
- strides : ant_sdm_common_data_t , ant_sdm_page1_data_t
- suported_new_alert_cat : ble_ans_c_service_t
- suported_unread_alert_cat : ble_ans_c_service_t
- supplementary_page_number : ant_sdm_sens_config_t
- support_notification : ble_bas_init_t
- supported_functions : ble_cs_ctrlpt_init_t , ble_sc_ctrlpt_s
- svc_num : nrf_svc_func_reg_t
- svci_num : nrf_svc_func_reg_t
- sw_rev_str : ble_dis_init_t
- sw_revision_major : ant_common_page81_data_t
- sw_revision_minor : ant_common_page81_data_t
- sw_version : ant_hrm_page3_data_t , ant_bsc_page3_data_t
- system_time : antfs_dir_header_t