| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_cscs_meas_s Struct Reference
Cycling Speed and Cadence Service

Cycling Speed and Cadence Service measurement structure. This contains a Cycling Speed and Cadence Service measurement. More...

`#include <ble_cscs.h>`

## Data Fields
bool | is_wheel_rev_data_present
bool | is_crank_rev_data_present
uint32_t | cumulative_wheel_revs
uint16_t | last_wheel_event_time
uint16_t | cumulative_crank_revs
uint16_t | last_crank_event_time

## Detailed Description

Cycling Speed and Cadence Service measurement structure. This contains a Cycling Speed and Cadence Service measurement.

## Field Documentation

uint16_t ble_cscs_meas_s::cumulative_crank_revs

Cumulative Crank Revolutions.

uint32_t ble_cscs_meas_s::cumulative_wheel_revs

Cumulative Wheel Revolutions.

bool ble_cscs_meas_s::is_crank_rev_data_present

True if Crank Revolution Data is present in the measurement.

bool ble_cscs_meas_s::is_wheel_rev_data_present

True if Wheel Revolution Data is present in the measurement.

uint16_t ble_cscs_meas_s::last_crank_event_time

Last Crank Event Time.

uint16_t ble_cscs_meas_s::last_wheel_event_time

Last Wheel Event Time.