| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Address types
Defines

## Macros
#define | BLE_GAP_ADDR_TYPE_PUBLIC 0x00
#define | BLE_GAP_ADDR_TYPE_RANDOM_STATIC 0x01
#define | BLE_GAP_ADDR_TYPE_RANDOM_PRIVATE_RESOLVABLE 0x02
#define | BLE_GAP_ADDR_TYPE_RANDOM_PRIVATE_NON_RESOLVABLE 0x03

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_ADDR_TYPE_PUBLIC 0x00

Public address.

#define BLE_GAP_ADDR_TYPE_RANDOM_PRIVATE_NON_RESOLVABLE 0x03

Private Non-Resolvable address.

#define BLE_GAP_ADDR_TYPE_RANDOM_PRIVATE_RESOLVABLE 0x02

Private Resolvable address.

#define BLE_GAP_ADDR_TYPE_RANDOM_STATIC 0x01

Random Static address.