| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_uuid_t Struct Reference
Structures

Bluetooth Low Energy UUID type, encapsulates both 16-bit and 128-bit UUIDs. More...

`#include <ble_types.h>`

## Data Fields
uint16_t | uuid
uint8_t | type

## Detailed Description

Bluetooth Low Energy UUID type, encapsulates both 16-bit and 128-bit UUIDs.

## Field Documentation

uint8_t ble_uuid_t::type

UUID type, see Types of UUID. If type is BLE_UUID_TYPE_UNKNOWN, the value of uuid is undefined.

uint16_t ble_uuid_t::uuid

16-bit UUID value or octets 12-13 of 128-bit UUID.