| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_evt_connected_t Struct Reference
Structures

Event structure for BLE_GAP_EVT_CONNECTED. More...

`#include <ble_gap.h>`

## Data Fields
ble_gap_addr_t | peer_addr
uint8_t | role
ble_gap_conn_params_t | conn_params

## Detailed Description

Event structure for BLE_GAP_EVT_CONNECTED.

## Field Documentation

ble_gap_conn_params_t ble_gap_evt_connected_t::conn_params

GAP Connection Parameters.

ble_gap_addr_t ble_gap_evt_connected_t::peer_addr

                  Bluetooth address of the peer device. If the peer_addr resolved: @ref ble_gap_addr_t::addr_id_peer is set to 1

and the address is the device's identity address.

uint8_t ble_gap_evt_connected_t::role

BLE role for this connection, see GAP Roles