| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_evt_passkey_display_t Struct Reference
Structures

Event structure for BLE_GAP_EVT_PASSKEY_DISPLAY. More...

`#include <ble_gap.h>`

## Data Fields
uint8_t | passkey [6]
uint8_t | match_request: 1

## Detailed Description

Event structure for BLE_GAP_EVT_PASSKEY_DISPLAY.

## Field Documentation

uint8_t ble_gap_evt_passkey_display_t::match_request

                     If 1 requires the application to report the match using @ref sd_ble_gap_auth_key_reply

with either BLE_GAP_AUTH_KEY_TYPE_NONE if there is no match or BLE_GAP_AUTH_KEY_TYPE_PASSKEY if there is a match.

uint8_t ble_gap_evt_passkey_display_t::passkey[6]

6-digit passkey in ASCII ('0'-'9' digits only).