| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_drv_gpiote_in_config_t Struct Reference
GPIOTE driver

Input pin configuration. More...

`#include <nrf_drv_gpiote.h>`

## Data Fields
nrf_gpiote_polarity_t | sense
nrf_gpio_pin_pull_t | pull
bool | is_watcher
bool | hi_accuracy

## Detailed Description

Input pin configuration.

## Field Documentation

bool nrf_drv_gpiote_in_config_t::hi_accuracy

True when high accuracy (IN_EVENT) is used.

bool nrf_drv_gpiote_in_config_t::is_watcher

True when the input pin is tracking an output pin.

nrf_gpio_pin_pull_t nrf_drv_gpiote_in_config_t::pull

Pulling mode.

nrf_gpiote_polarity_t nrf_drv_gpiote_in_config_t::sense

Transition that triggers interrupt.