| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_gzll_host_rx_info_t Struct Reference
Gazell Link Layer

Data structure containing information about the last packet received. More...

`#include <nrf_gzll.h>`

## Data Fields
bool | packet_removed_from_tx_fifo
| A payload was received in the ACK.
int16_t | rssi
| Received signal strength indicator in dBm. More...

## Detailed Description

Data structure containing information about the last packet received.

## Field Documentation

int16_t nrf_gzll_host_rx_info_t::rssi

Received signal strength indicator in dBm.

See Also
  nrf_gzll_enable_rssi().