| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_cts_c_s Struct Reference
Current Time Service client

Current Time Service client structure. This structure contains status information for the client. More...

`#include <ble_cts_c.h>`

## Data Fields
ble_cts_c_evt_handler_t | evt_handler
ble_srv_error_handler_t | error_handler
ble_cts_c_handles_t | char_handles
uint16_t | conn_handle

## Detailed Description

Current Time Service client structure. This structure contains status information for the client.

## Field Documentation

ble_cts_c_handles_t ble_cts_c_s::char_handles

Handles of Current Time Characteristic at the peer (handles are provided by the BLE stack through the DB Discovery module).

uint16_t ble_cts_c_s::conn_handle

Handle of the current connection. BLE_CONN_HANDLE_INVALID if not in a connection.

ble_srv_error_handler_t ble_cts_c_s::error_handler

Function to be called if an error occurs.

ble_cts_c_evt_handler_t ble_cts_c_s::evt_handler

Event handler to be called for handling events from the Current Time Service client.