| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
antfs_params_t Struct Reference
ANT-FS client device simulator

ANT-FS parameters. More...

`#include <antfs.h>`

## Data Fields
uint32_t | client_serial_number
uint16_t | beacon_device_type
uint16_t | beacon_device_manufacturing_id
uint8_t | beacon_frequency
antfs_beacon_status_byte1_t | beacon_status_byte1
const uint8_t * | p_pass_key
const uint8_t * | p_remote_friendly_name

## Detailed Description

ANT-FS parameters.

## Field Documentation

uint16_t antfs_params_t::beacon_device_manufacturing_id

Client manufacturing ID.

uint16_t antfs_params_t::beacon_device_type

Client device type.

uint8_t antfs_params_t::beacon_frequency

Beacon RF Frequency.

antfs_beacon_status_byte1_t antfs_params_t::beacon_status_byte1

Beacon status byte 1.

uint32_t antfs_params_t::client_serial_number

Client serial number.

const uint8_t* antfs_params_t::p_pass_key

Pass Key.

const uint8_t* antfs_params_t::p_remote_friendly_name

Friendly Name.