| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_ble_bms_s Struct Reference
Bond Management Service

Status information for the service. More...

`#include <nrf_ble_bms.h>`

## Data Fields
uint16_t | service_handle
| Handle of the Bond Management Service (as provided by the BLE stack).
uint16_t | conn_handle
| Handle of the current connection (as provided by the BLE stack). BLE_CONN_HANDLE_INVALID if not in a connection.
ble_bms_evt_handler_t | evt_handler
| Event handler to be called for handling events in the Bond Management Service.
ble_srv_error_handler_t | error_handler
| Function to be called if an error occurs.
nrf_ble_bms_features_t | feature
| Value for features of the service (see BMS feature bits).
ble_gatts_char_handles_t | feature_handles
| Handles related to the Bond Management Feature characteristic.
ble_gatts_char_handles_t | ctrlpt_handles
| Handles related to the Bond Management Control Point characteristic.
nrf_ble_bms_bond_cbs_t | bond_callbacks
| Callback functions for deleting bonds.
nrf_ble_bms_auth_status_t | auth_status
| Authorization status.

## Detailed Description

Status information for the service.