| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Modules
Heart Rate Service Client
BLE Services

Heart Rate Service Client module. More...

## Modules
| Enumerations
| Structures
| Types
| Functions
| Heart Rate Service Client configuration

## Detailed Description

Heart Rate Service Client module.

This module contains the APIs and types exposed by the Heart Rate Service Client module. These APIs and types can be used by the application to perform discovery of Heart Rate Service at the peer and interact with it.

Warning
  Currently this module only has support for Heart Rate Measurement characteristic. This means that it will be able to enable notification of the characteristic at the peer and be able to receive Heart Rate Measurement notifications from the peer. It does not support the Body Sensor Location and the Heart Rate Control Point characteristics. When a Heart Rate Measurement is received, this module will decode only the Heart Rate Measurement Value (both 8 bit and 16 bit) field from it and provide it to the application.

Note
  The application must propagate BLE stack events to this module by calling ble_hrs_c_on_ble_evt().