| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
SVC return values specific to GAP
Defines

## Macros
#define | BLE_ERROR_GAP_UUID_LIST_MISMATCH (NRF_GAP_ERR_BASE + 0x000)
#define | BLE_ERROR_GAP_DISCOVERABLE_WITH_WHITELIST (NRF_GAP_ERR_BASE + 0x001)
#define | BLE_ERROR_GAP_INVALID_BLE_ADDR (NRF_GAP_ERR_BASE + 0x002)
#define | BLE_ERROR_GAP_WHITELIST_IN_USE (NRF_GAP_ERR_BASE + 0x003)
#define | BLE_ERROR_GAP_DEVICE_IDENTITIES_IN_USE (NRF_GAP_ERR_BASE + 0x004)
#define | BLE_ERROR_GAP_DEVICE_IDENTITIES_DUPLICATE (NRF_GAP_ERR_BASE + 0x005)

## Detailed Description

## Macro Definition Documentation

#define BLE_ERROR_GAP_DEVICE_IDENTITIES_DUPLICATE (NRF_GAP_ERR_BASE + 0x005)

The device identity list contains entries with duplicate identity addresses.

#define BLE_ERROR_GAP_DEVICE_IDENTITIES_IN_USE (NRF_GAP_ERR_BASE + 0x004)

Attempt to modify the device identity list while already in use by another operation.

#define BLE_ERROR_GAP_DISCOVERABLE_WITH_WHITELIST (NRF_GAP_ERR_BASE + 0x001)

Use of Whitelist not permitted with discoverable advertising.

#define BLE_ERROR_GAP_INVALID_BLE_ADDR (NRF_GAP_ERR_BASE + 0x002)

The upper two bits of the address do not correspond to the specified address type.

#define BLE_ERROR_GAP_UUID_LIST_MISMATCH (NRF_GAP_ERR_BASE + 0x000)

UUID list does not contain an integral number of UUIDs.

#define BLE_ERROR_GAP_WHITELIST_IN_USE (NRF_GAP_ERR_BASE + 0x003)

Attempt to modify the whitelist while already in use by another operation.