| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Application timer functionality configuration
Application Timer

## Macros
#define | APP_TIMER_ENABLED
| Enabling app_timer module * Set to 1 to activate. More...
#define | APP_TIMER_WITH_PROFILER
| Enable app_timer profiling * Set to 1 to activate. More...
#define | APP_TIMER_KEEPS_RTC_ACTIVE
| Enable RTC always on. More...

## Detailed Description

## Macro Definition Documentation

#define APP_TIMER_ENABLED

Enabling app_timer module * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define APP_TIMER_KEEPS_RTC_ACTIVE

Enable RTC always on.

If option is enabled RTC is kept running even if there is no active timers. This option can be used when app_timer is used for timestamping.

Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define APP_TIMER_WITH_PROFILER

Enable app_timer profiling * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.