| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Defines
Master Boot Record API

## Macros
#define | MBR_SVC_BASE (0x18)
| MBR SVC Base number.
#define | MBR_PAGE_SIZE_IN_WORDS (1024)
| Page size in words.
#define | MBR_SIZE (0x1000)
| The size that must be reserved for the MBR when a softdevice is written to flash. This is the offset where the first byte of the softdevice hex file is written.

## Detailed Description