| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gatts_hvx_params_t Struct Reference
Structures

GATT HVx parameters. More...

`#include <ble_gatts.h>`

## Data Fields
uint16_t | handle
uint8_t | type
uint16_t | offset
uint16_t * | p_len
uint8_t * | p_data

## Detailed Description

GATT HVx parameters.

## Field Documentation

uint16_t ble_gatts_hvx_params_t::handle

Characteristic Value Handle.

uint16_t ble_gatts_hvx_params_t::offset

Offset within the attribute value.

uint8_t* ble_gatts_hvx_params_t::p_data

Actual data content, use NULL to use the current attribute value.

uint16_t* ble_gatts_hvx_params_t::p_len

Length in bytes to be written, length in bytes written after successful return.

uint8_t ble_gatts_hvx_params_t::type

Indication or Notification, see GATT Handle Value operations.