| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Enumerations
Enumerations
Generic Attribute Profile (GATT) Client

## Enumerations
enum | BLE_GATTC_SVCS { SD_BLE_GATTC_PRIMARY_SERVICES_DISCOVER = 0x90, SD_BLE_GATTC_RELATIONSHIPS_DISCOVER, SD_BLE_GATTC_CHARACTERISTICS_DISCOVER, SD_BLE_GATTC_DESCRIPTORS_DISCOVER, SD_BLE_GATTC_ATTR_INFO_DISCOVER, SD_BLE_GATTC_CHAR_VALUE_BY_UUID_READ, SD_BLE_GATTC_READ, SD_BLE_GATTC_CHAR_VALUES_READ, SD_BLE_GATTC_WRITE, SD_BLE_GATTC_HV_CONFIRM }
| GATTC API SVC numbers. More...
enum | BLE_GATTC_EVTS { BLE_GATTC_EVT_PRIM_SRVC_DISC_RSP = 0x30, BLE_GATTC_EVT_REL_DISC_RSP, BLE_GATTC_EVT_CHAR_DISC_RSP, BLE_GATTC_EVT_DESC_DISC_RSP, BLE_GATTC_EVT_ATTR_INFO_DISC_RSP, BLE_GATTC_EVT_CHAR_VAL_BY_UUID_READ_RSP, BLE_GATTC_EVT_READ_RSP, BLE_GATTC_EVT_CHAR_VALS_READ_RSP, BLE_GATTC_EVT_WRITE_RSP, BLE_GATTC_EVT_HVX, BLE_GATTC_EVT_TIMEOUT }
| GATT Client Event IDs. More...

## Detailed Description

## Enumeration Type Documentation

enum BLE_GATTC_EVTS

GATT Client Event IDs.

Enumerator
BLE_GATTC_EVT_PRIM_SRVC_DISC_RSP | GATTC BLE Event base. Primary Service Discovery Response event. See ble_gattc_evt_prim_srvc_disc_rsp_t.
BLE_GATTC_EVT_REL_DISC_RSP | Relationship Discovery Response event. See ble_gattc_evt_rel_disc_rsp_t.
BLE_GATTC_EVT_CHAR_DISC_RSP | Characteristic Discovery Response event. See ble_gattc_evt_char_disc_rsp_t.
BLE_GATTC_EVT_DESC_DISC_RSP | Descriptor Discovery Response event. See ble_gattc_evt_desc_disc_rsp_t.
BLE_GATTC_EVT_ATTR_INFO_DISC_RSP | Attribute Information Response event. See ble_gattc_evt_attr_info_disc_rsp_t.
BLE_GATTC_EVT_CHAR_VAL_BY_UUID_READ_RSP | Read By UUID Response event. See ble_gattc_evt_char_val_by_uuid_read_rsp_t.
BLE_GATTC_EVT_READ_RSP | Read Response event. See ble_gattc_evt_read_rsp_t.
BLE_GATTC_EVT_CHAR_VALS_READ_RSP | Read multiple Response event. See ble_gattc_evt_char_vals_read_rsp_t.
BLE_GATTC_EVT_WRITE_RSP | Write Response event. See ble_gattc_evt_write_rsp_t.
BLE_GATTC_EVT_HVX | Handle Value Notification or Indication event. Confirm indication with sd_ble_gattc_hv_confirm. See ble_gattc_evt_hvx_t.
BLE_GATTC_EVT_TIMEOUT | Timeout event. See ble_gattc_evt_timeout_t.

enum BLE_GATTC_SVCS

GATTC API SVC numbers.

Enumerator
SD_BLE_GATTC_PRIMARY_SERVICES_DISCOVER | GATTC BLE SVC base. Primary Service Discovery.
SD_BLE_GATTC_RELATIONSHIPS_DISCOVER | Relationship Discovery.
SD_BLE_GATTC_CHARACTERISTICS_DISCOVER | Characteristic Discovery.
SD_BLE_GATTC_DESCRIPTORS_DISCOVER | Characteristic Descriptor Discovery.
SD_BLE_GATTC_ATTR_INFO_DISCOVER | Attribute Information Discovery.
SD_BLE_GATTC_CHAR_VALUE_BY_UUID_READ | Read Characteristic Value by UUID.
SD_BLE_GATTC_READ | Generic read.
SD_BLE_GATTC_CHAR_VALUES_READ | Read multiple Characteristic Values.
SD_BLE_GATTC_WRITE | Generic write.
SD_BLE_GATTC_HV_CONFIRM | Handle Value Confirmation.