| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_ble_bms_init_t Struct Reference
Bond Management Service

BMS initialization structure that contains all information needed to initialize the service. More...

`#include <nrf_ble_bms.h>`

## Data Fields
ble_bms_evt_handler_t | evt_handler
| Event handler to be called for handling events in the Bond Management Service.
ble_srv_error_handler_t | error_handler
| Function to be called if an error occurs.
nrf_ble_bms_features_t | feature
| Initial value for features of the service.
security_req_t | bms_feature_sec_req
| Initial security level for the Feature characteristic.
security_req_t | bms_ctrlpt_sec_req
| Initial security level for the Control Point characteristic.
nrf_ble_qwr_t * | p_qwr
| Pointer to the initialized Queued Write context.
nrf_ble_bms_bond_cbs_t | bond_callbacks
| Callback functions for deleting bonds.

## Detailed Description

BMS initialization structure that contains all information needed to initialize the service.