| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_dfu_res_t Struct Reference
Request handling

Response used during DFU operations. More...

`#include <nrf_dfu_req_handler.h>`

## Data Fields
union {
struct {
uint8_t * p_res
uint32_t res_len
} |
struct {
uint32_t max_size
uint32_t offset
uint32_t crc
} |
}; |

## Detailed Description

Response used during DFU operations.

## Field Documentation

uint32_t nrf_dfu_res_t::crc

Current CRC.

uint32_t nrf_dfu_res_t::max_size

Maximum size of the object of a given type.

uint32_t nrf_dfu_res_t::offset

Current offset.

uint8_t* nrf_dfu_res_t::p_res

Pointer to an array holding the serialized version of the response.

uint32_t nrf_dfu_res_t::res_len

Length of the response array.